---
name: Bug report
about: Create a report to help us improve
title: ''
labels: ''
assignees: ''

---

### Describe the bug

A clear and concise description of what the bug is.

### Steps to Reproduce

Steps to reproduce the behavior. Including the [MRE](https://stackoverflow.com/help/minimal-reproducible-example) sketches

### Expected behavior

A clear and concise description of what you expected to happen.

### Actual behavior

A clear and concise description of what you expected to happen.

### Debug and AT-command log (if applicable)

A clear and concise description of what you expected to happen.

### Screenshots

If applicable, add screenshots to help explain your problem.

---

### Information

Please ensure to specify the following:

* Arduino IDE version (e.g. 1.8.19) or Platform.io version
* `RP2040` Core Version (e.g. RP2040 core v2.7.1)
* `RP2040` Board type (e.g. RASPBERRY_PI_PICO_W)
* Contextual information (e.g. what you were trying to achieve)
* Simplest possible steps to reproduce
* Anything that might be relevant in your opinion, such as:
  * Operating system (Windows, Ubuntu, etc.) and the output of `uname -a`
  * Network configuration


Please be educated, civilized and constructive as you've always been. Disrespective posts against [GitHub Code of Conduct](https://docs.github.com/en/site-policy/github-terms/github-event-code-of-conduct) will be ignored and deleted.

---

### Example

```
Arduino IDE version: 1.8.19
RP2040 core v2.7.1
RASPBERRY_PI_PICO_W Module
OS: Ubuntu 20.04 LTS
Linux xy-Inspiron-3593 5.15.0-58-generic #64~20.04.1-Ubuntu SMP Fri Jan 6 16:42:31 UTC 2023 x86_64 x86_64 x86_64 GNU/Linux

Context:
I encountered a crash while using this library

Steps to reproduce:
1. ...
2. ...
3. ...
4. ...
```

### Additional context

Add any other context about the problem here.

