
/* ULP variable definitions for the linker.
 * This file is generated automatically by esp32ulp_mapgen.py utility.
 */
PROVIDE ( ulp_battery_adc_value = 0x50000440 );
PROVIDE ( ulp_button_counter = 0x50000304 );
PROVIDE ( ulp_ch0_adc_value = 0x50000438 );
PROVIDE ( ulp_ch0_pulse_count = 0x50000428 );
PROVIDE ( ulp_ch0_read = 0x50000034 );
PROVIDE ( ulp_ch0_type = 0x50000430 );
PROVIDE ( ulp_ch1_adc_value = 0x5000043c );
PROVIDE ( ulp_ch1_pulse_count = 0x5000042c );
PROVIDE ( ulp_ch1_read = 0x50000190 );
PROVIDE ( ulp_ch1_type = 0x50000434 );
PROVIDE ( ulp_check_wake_up = 0x50000308 );
PROVIDE ( ulp_entry = 0x50000000 );
PROVIDE ( ulp_exit = 0x500003dc );
PROVIDE ( ulp_input = 0x5000044c );
PROVIDE ( ulp_stop_and_exit = 0x500003e0 );
PROVIDE ( ulp_use_led = 0x50000444 );
PROVIDE ( ulp_use_out = 0x50000448 );
PROVIDE ( ulp_wake_up = 0x500003e8 );
PROVIDE ( ulp_wake_up_counter = 0x500002fc );
PROVIDE ( ulp_wake_up_event = 0x50000300 );
PROVIDE ( ulp_wake_up_period = 0x500002f8 );
