
/* ULP variable definitions for the linker.
 * This file is generated automatically by esp32ulp_mapgen.py utility.
 */
PROVIDE ( ulp_battery_adc_value = 0x500003c0 );
PROVIDE ( ulp_ch0_adc_value = 0x500003b8 );
PROVIDE ( ulp_ch0_pulse_count = 0x500003a8 );
PROVIDE ( ulp_ch0_read = 0x50000034 );
PROVIDE ( ulp_ch0_type = 0x500003b0 );
PROVIDE ( ulp_ch1_adc_value = 0x500003bc );
PROVIDE ( ulp_ch1_pulse_count = 0x500003ac );
PROVIDE ( ulp_ch1_read = 0x5000016c );
PROVIDE ( ulp_ch1_type = 0x500003b4 );
PROVIDE ( ulp_check_wake_up = 0x500002e4 );
PROVIDE ( ulp_entry = 0x50000000 );
PROVIDE ( ulp_exit = 0x5000035c );
PROVIDE ( ulp_input = 0x500003cc );
PROVIDE ( ulp_stop_and_exit = 0x50000360 );
PROVIDE ( ulp_use_led = 0x500003c4 );
PROVIDE ( ulp_use_out = 0x500003c8 );
PROVIDE ( ulp_wake_up = 0x50000368 );
PROVIDE ( ulp_wake_up_counter = 0x500002dc );
PROVIDE ( ulp_wake_up_event = 0x500002e0 );
PROVIDE ( ulp_wake_up_period = 0x500002d8 );
