# List of supported OIDs
RNDIS_OID_GEN_SUPPORTED_LIST="\x00\x01\x01\x01"
# Hardware status
RNDIS_OID_GEN_HARDWARE_STATUS="\x00\x01\x01\x02"
# Media types supported (encoded)
RNDIS_OID_GEN_MEDIA_SUPPORTED="\x00\x01\x01\x03"
# Media types in use (encoded)
RNDIS_OID_GEN_MEDIA_IN_USE="\x00\x01\x01\x04"
RNDIS_OID_GEN_MAXIMUM_LOOKAHEAD="\x00\x01\x01\x05"
# Maximum frame size in bytes
RNDIS_OID_GEN_MAXIMUM_FRAME_SIZE="\x00\x01\x01\x06"
# Link speed in units of 100 bps
RNDIS_OID_GEN_LINK_SPEED="\x00\x01\x01\x07"
# Transmit buffer space
RNDIS_OID_GEN_TRANSMIT_BUFFER_SPACE="\x00\x01\x01\x08"
# Receive buffer space
RNDIS_OID_GEN_RECEIVE_BUFFER_SPACE="\x00\x01\x01\x09"
# NDIS version number used by the driver
RNDIS_OID_GEN_DRIVER_VERSION="\x00\x01\x01\x10"
# Maximum total packet length in bytes
RNDIS_OID_GEN_MAXIMUM_TOTAL_SIZE="\x00\x01\x01\x11"
# Optional protocol flags (encoded)
RNDIS_OID_GEN_PROTOCOL_OPTIONS="\x00\x01\x01\x12"
# Optional NIC flags (encoded)
RNDIS_OID_GEN_MAC_OPTIONS="\x00\x01\x01\x13"
# Whether the NIC is connected to the network
RNDIS_OID_GEN_MEDIA_CONNECT_STATUS="\x00\x01\x01\x14"
# The maximum number of send packets the driver can accept per call to its MiniportSendPacketsfunction
RNDIS_OID_GEN_MAXIMUM_SEND_PACKETS="\x00\x01\x01\x15"
# Vendor-assigned version number of the driver
RNDIS_OID_GEN_VENDOR_DRIVER_VERSION="\x00\x01\x01\x16"
# The custom GUIDs (Globally Unique Identifier) supported by the miniport driver
RNDIS_OID_GEN_SUPPORTED_GUIDS="\x00\x01\x01\x17"
# List of network-layer addresses associated with the binding between a transport and the driver
RNDIS_OID_GEN_NETWORK_LAYER_ADDRESSES="\x00\x01\x01\x18"
# Size of packets' additional headers
RNDIS_OID_GEN_TRANSPORT_HEADER_OFFSET="\x00\x01\x01\x19"
RNDIS_OID_GEN_MEDIA_CAPABILITIES="\x00\x01\x02\x01"
# Physical media supported by the miniport driver (encoded)
RNDIS_OID_GEN_PHYSICAL_MEDIUM="\x00\x01\x02\x02"
# Permanent station address
RNDIS_OID_802_3_PERMANENT_ADDRESS="\x01\x01\x01\x01"
# Current station address
RNDIS_OID_802_3_CURRENT_ADDRESS="\x01\x01\x01\x02"
# Current multicast address list
RNDIS_OID_802_3_MULTICAST_LIST="\x01\x01\x01\x03"
# Maximum size of multicast address list
RNDIS_OID_802_3_MAXIMUM_LIST_SIZE="\x01\x01\x01\x04"
# Directed packets. Directed packets contain a destination address equal to the station address of the NIC.
RNDIS_PACKET_TYPE_DIRECTED="\x00\x00\x00\x01"
# Multicast address packets sent to addresses in the multicast address list.
RNDIS_PACKET_TYPE_MULTICAST="\x00\x00\x00\x02"
# All multicast address packets, not just the ones enumerated in the multicast address list.
RNDIS_PACKET_TYPE_ALL_MULTICAST="\x00\x00\x00\x04"
# Broadcast packets.
RNDIS_PACKET_TYPE_BROADCAST="\x00\x00\x00\x08"
# All source routing packets. If the protocol driver sets this bit, the NDIS library attempts to act as a source routing bridge.
RNDIS_PACKET_TYPE_SOURCE_ROUTING="\x00\x00\x00\x10"
# Specifies all packets regardless of whether VLAN filtering is enabled or not and whether the VLAN identifier matches or not.
RNDIS_PACKET_TYPE_PROMISCUOUS="\x00\x00\x00\x20"
# SMT packets that an FDDI NIC receives.
RNDIS_PACKET_TYPE_SMT="\x00\x00\x00\x40"
# All packets sent by installed protocols and all packets indicated by the NIC that is identified by a given NdisBindingHandle.
RNDIS_PACKET_TYPE_ALL_LOCAL="\x00\x00\x00\x80"
# Packets sent to the current group address.
RNDIS_PACKET_TYPE_GROUP="\x00\x00\x10\x00"
# All functional address packets, not just the ones in the current functional address.
RNDIS_PACKET_TYPE_ALL_FUNCTIONAL="\x00\x00\x20\x00"
# Functional address packets sent to addresses included in the current functional address.
RNDIS_PACKET_TYPE_FUNCTIONAL="\x00\x00\x40\x00"
# NIC driver frames that a Token Ring NIC receives.
RNDIS_PACKET_TYPE_MAC_FRAME="\x00\x00\x80\x00"
RNDIS_PACKET_TYPE_NO_LOCAL="\x00\x01\x00\x00"

